                                                 CSC-STD-004-85

              TECHNICAL RATIONAL BEHIND CSC-STD-003-85:
                   COMPUTER SECURITY REQUIREMENTS

              GUIDANCE FOR APPLYING THE DEPARTMENT OF DEFENSE
                TRUSTED COMPUTER SYSTEM EVALUATION CRITERIA
                         IN SPECIFIC ENVIRONMENTS

              Approved for public release;
              distribution unlimited.

              25 June 1985

                                                        CSC-STD-004-85
                                                 Library No. S-226,728

                                FOREWORD

This publication, Technical Rationale Behind CSC-STD-003-85: Computer Security
Requirements--Guidance for Applying the Department of Defense Trusted Computer
System Evaluation Criteria in Specific Environments, is being issued by the
DoD Computer Security Center (DoDCSC) under the authority of and in accordance
with DoD Directive 5215.1, "Computer Security Evaluation Center." This
document presents background discussion and rationale for CSC-STD-003-85,
Computer Security Requirements--Guidance for Applying the Department of
Defense Trusted Computer System Evaluation Criteria in Specific
Environments. The computer security requirements identify the minimum class of
system required for a given risk index. System classes are those defined by
CSC-STD-001-83, Department of Defense Trusted Computer System Evaluation
Criteria, 15 August 1983. Risk index is defined as the disparity between the
minimum clearance or authorization of system users and the maximum sensitivity
of data processed by the system. This guidance is intended to be used in
establishing minimum computer security requirements for the processing an-or
storage and retrieval of sensitive or classified information by the Department
of Defense whenever automatic data processing systems are employed. Point of
contact concerning this publication is the Office of Standards and Products,
Attention: Chief, Computer Security Standards.

                                 25 June 1985
Robert L. Brotzman
Director
DoD Computer Security Center

                                 ACKNOWLEDGMENTS

Special recognition is extended to H.  William Neugent and Ingrid M. Olson of
the MITRE Corporation for performing in-depth analysis of DoD policies and
procedures and for preparation of this document.

Acknowledgment is given to the following for formulating the computer security
requirements and the supporting technical and procedural rationale behind
these requirements: Col Roger R. Schell, formerly DoDCSC, George F. Jelen,
formerly DoDCSC, Daniel J. Edwards, Sheila L. Brand, and Stephen F. Barnett,
DoDCSC.

Acknowledgment is also given to the following for giving generously of their
time and expertise in the review and critique of this document: CDR Robert
Emery, OJCS, Dan Mechelke, 902nd Ml Gp, Mary Taylor, DAMI-CIC, Maj.  Freeman,
DAMI- CIC, Ralph Neeper, DAMI-CIC, Duane Fagg, NAVDAC, H.  O.  Lubbes,
NAVELEX, Sue Berg, OPNAV, Susan Tominack, NAVDAC, Lt Linda Fischer, OPNAV,
Eugene Epperly, ODUSD(P), Maj Grace Culver, USAF-SITT, Capt Mike Weidner,
ASPO, Alfred W. Arsenault, DoDCSC, James P.  Anderson, James P.  Anderson &
Co., and Dr. John Vasak, MITRE Corporation.

                             TABLE OF CONTENTS

FOREWORD.............................................................   i
ACKNOWLEDGMENTS......................................................  ii
LIST OF TABLES.......................................................  iv
1.0 INTRODUCTION.....................................................   1
2.0 RISE INDEX.......................................................   5
3.0 COMPUTER SECURITY REQUIREMENTS FOR OPEN
    SECURITY ENVIRONMENTS............................................   11
4.0 COMPUTER SECURITY REQUIREMENTS FOR CLOSED
    SECURITY ENVIRONMENTS............................................   19
APPENDIX A: SUMMARY OF CRITERIA......................................   23
APPENDIX B: DETAILED DESCRIPTION OF CLEARANCES
     AND DATA SENSITIVITIES..........................................   27
APPENDIX C: ENVIRONMENTAL TYPES......................................   31
GLOSSARY.............................................................   33
ACRONYMS.............................................................   37
REFERENCES...........................................................   39

                             LIST OF TABLES

Table
1: Rating Scale for Minimum User Clearance.........................    6
2: Rating Scale for Maximum Data Sensitivity.......................    7
3: Security Risk Index Matrix......................................    8
4: Computer Security Requirements for Open Security Environments...   12
5: Security Index Matrix for Open Security Environments............   13
6: Computer Security Requirements for Closed Security Environments.   20
7: Security Index Matrix for Closed Security Environments..........   21

 1.0 INTRODUCTION

The purpose of this technical report is to present background discussion and
rationale for Computer Security Requirements--Guidance for Applying the DoD
Trusted Computer System Evaluation Criteria in Specific Environments(1)
(henceforth referred to as the Computer Security Requirements).  The
requirements were prepared in compliance with responsibilities assigned to the
Department of Defense (DoD) Computer Security Center (DoDCSC) under DoD
Directive 5215.1, which tasks the DoDCSC to "establish and maintain technical
standards and criteria for the evaluation of trusted computer systems."(2)

DoD computer systems have stringent requirements for security. In the past,
these requirements have been satisfied primarily through physical, personnel,
and information security safeguards.(3) Recent advances in technology make it
possible to place increasing trust in the computer system itself, thereby
increasing security effectiveness and efficiency. In turn, the need has arisen
for guidance on how this new technology should be used. There are two facets
to this required guidance:

     a.  Establishment of a metric for categorizing systems according to the
         security protection they provide.

     b.  Identification of the minimum security protection required in
         different environments.

The DoD Trusted Computer System Evaluation Criteria (henceforth referred to
as the Criteria), developed by the DoDCSC, satisfy the first of these two
requirements by categorizing computer systems into hierarchical security
classes.(4) The Computer Security Requirements satisfy the second requirement
by identifying the minimum classes appropriate for systems in different risk
environments. They are to be used by system managers in applying the Criteria
and thereby in selecting and specifying systems that have sufficient security
protection for specific operational environments.

Section 2 of this document discusses the risk index.  Section 3 presents a
discussion of the Computer Security Requirements for open security
environments.  Section 4 presents a discussion of the Computer Security
Requirements for closed security environments. A summary of the Criteria is
contained in Appendix A.  Appendix B contains a detailed description of
clearances and data sensitivities, and Appendix C describes the environmental
types.  A glossary provides definitions of many of the terms used in this
document.

1.1 Scope and Applicability

This section describes the scope and applicability for both this report and
the Computer Security Requirements. The primary focus of both documents is
on the technical aspects (e.g., hardware, software, configuration control)
of computer security, although the two documents also address the relationship
between computer security and physical, personnel, and information
security.  While communications and emanations security are important elements
of system security, they are outside the scope of the two documents.

Both documents apply to DoD computer systems that are entrusted with the
protection of information, regardless of whether or not that information is
classified, sensitive, national security-related, or any combination thereof.
Furthermore, both documents can be applied throughout the DoD.(5,6,7,8,9)

The two documents are concerned with protection against both disclosure and
integrity violations. Integrity violations are of particular concern for
sensitive unclassified information (e.g., financial data) as well as for some
classified applications (e.g., missile guidance data).

The recommendations of both this report and the Computer Security
Requirements are stated in terms of classes from the Criteria. Embodied in
each class and therefore encompassed within the scope of both documents are
two types of requirements:  assurance and feature requirements.  Assurance
requirements are those that contribute to confidence that the required
features are present and that the system is functioning as intended.  Examples
of assurance requirements include modular design, penetration testing, formal
verification, and trusted configuration management.  Feature requirements
encompass capabilities such as labeling, authentication, and auditing.

1.2 Security Operating Modes

DoD computer security policy identifies several security operating modes, for
which the following definitions are adapted:(10,11,12,13)

     a.  Dedicated Security Mode--The mode of operation in which the system is
         specifically and exclusively dedicated to and controlled for the
         processing of one particular type or classification of information,
         either for fulltime operation or for a specified period of time.

     b.  System High Security Mode--The mode of operation in which system
         hardware/software is only trusted to provide need-to-know protection
         between users.  In this mode, the entire system, to include all
         components electrically and/or physically connected, must operate
         with security measures commensurate with the highest classification
         and sensitivity of the information being processed and/or stored.
         All system users in this environment must possess clearances and
         authorizations for all information contained in the system, and all
         system output must be clearly marked with the highest classification
         and all system caveats, until the information has been reviewed
         manually by an authorized individual to ensure appropriate
         classifications and caveats have been affixed.

     c.  Multilevel Security Mode--The mode of operation which allows two or
         more classification levels of information to be processed
         simultaneously within the same system when some users are not cleared
         for all levels of information present.

     d.  Controlled Mode--The mode of operation that is a type of multilevel
         security in which a more limited amount of trust is placed in the
         hardware/software base of the system, with resultant restrictions on
         the classification levels and clearance levels that may be supported.

     e.  Compartmented Security Mode--The mode of operation which allows
         the system to process two or more types of compartmented information

         (information requiring a special authorization) or any one type of
         compartmented information with other than compartmented information.
         In this mode, system access is secured to at least the Top Secret
         (TS) level, but all system users need not necessarily be formally
         authorized access to all types of compartmented information being
         processed and/or stored in the system.

In addition to these security operating modes, Service policies may define
other modes of operation.  For example, Office of the Chief of Naval
Operations (OPNAV) Instruction 5239.  IA defines Limited Access Mode for those
systems in which the minimum user clearance is uncleared and the maximum
data sensitivity is not classified but sensitive (6)

2.0 RISK INDEX

The evaluation class appropriate for a system is dependent on the level of
security risk inherent to that system.  This inherent risk is referred to as
that systems risk index.  Risk index is defined as follows:

     The disparity between the minimum clearance or authorization of system
     users and the maximum sensitivity of data processed by a system.

The Computer Security Requirements are based upon this risk index.  Although
there are other factors that can influence security risk, such as mission
criticality, required denial of service protection, and threat severity, only
the risk index is used to determine the minimum class of trusted systems to be
employed, since it can be uniformly applied in the determination of security
risk.  The risk index for a system depends on the rating associated with the
system's mimimum user clearance (Rmin) taken from Table 1 and the rating
associated with the system's maximum data sensitivity (Rmax) taken from Table

2.  The risk index is computed as follows:

Case a. If Rmin is less than Rmax, then the risk index is determined by
subtracting Rmin from Rmax.2
                        Risk Index  Rmax   Rmin

Case b. If Rmin is greater than or equal to Rmax, then
                1, if there are categories on the system to which some users
                   are not authorized access;
Risk Index
                0, otherwise (i.e., if there are no categories on the system
                   or if all users are authorized access to all categories)

     Example: For a system with a minimum user clearance of Confidential and
     maximum data sensititivy of Secret (without categories), Rmin 2 and
     Rmax 3.

1 Since a clearance implicitly encompasses lower clearance levels (e.g., a
Secret- cleared user has an implicit Confidential clearance), the phrase
"minimum clearance...of system users" is more accurately stated as "maximum
clearance of the least cleared system user." For simplicity, this document
uses the former phrase.

2 There is one anomalous case in which this formula gives an incorrect result
This is the case where the minimum clearance is Top Secret/Background
Investigation and the maximum data sensitivity is Top Secret. According to
the formula, this gives a risk index of l. In actuality, the risk index in
this case is zero. The anomaly results because there are two "levels" of Top
Secret clearance and only one level of Top Secret data.

       RATING SCALE FOR MINIMUM USER CLEARANCE1

            MINIMUM USER CLEARANCE                                RATING

                      Uncleared (U)                                  0

   Not Cleared but Authorized Access to Sensitive Unclassified       1
                     Information (N)
                     Confidential (C)                                2
                        Secret(S)                                    3
     Top Secret (TS)/Current Background Investigation (BI)           4
 Top Secret (TS)/Current Special Background Investigation (SBI)      5
                One Category (1C)                                    6
              Multiple Categories (MC)                               7

1 See Appendix B for a detailed description of the terms listed

                       TABLE 2

      RATING SCALE FOR MAXIMUM DATA SENSITIVITY

 MAXIMUM DATA
  SENSITIVITY
  RATINGS 2         RATING   MAXIMUM DATA SENSITIVITY WITH
    WITHOUT         (Rmax)        CATEGORIES1
  CATEGORIES
     (Rmax)

 Unclassified (U)      0          Not Applicable3
Not Classified but     1     N With One or More Categories            2
     Sensitives4
 Confidential (C)      2     C With One or More Categories            3
   Secret(S)           3     S With One or More Categories With No    4
                               More Than One Category Containing
                               Secret Data
                             S With Two or More Categories Containing 5
                               Secret Data
 Top Secret (TS)       55    TS With One or More Categories With No   6
                             More Than One Category Containing
                             Secret or Top Secret Data
                             TS With Two or More Categories           7
                             Containing Secret or Top Secret Data

1 The only categories of concern are those for which some users are not
authorized access to the category.  When counting the number of categories,
count all categories regardless of the sensitivity level associated with the
data.  If a category is associated with more than one sensitivity level, it is
only counted at the highest level.

2 Where the number of categories is large or where a highly sensitive category
is involved, a higher rating might be warranted.

3 Since categories imply sensitivity of data and unclassified data is not
sensitive, unclassified data by definition cannot contain categories.

4 N data includes financial, proprietary, privacy, and mission sensitive data.
Some situations (e.g., those involving extremely large financial sums or
critical mission sensitive data), may warrant a higher rating.  The table
prescribes minimum ratings

5 The rating increment between the Secret and Top Secret data sensitivity
levels is greater than the increment between other adjacent levels.  This
difference derives from the fact that the loss of Top Secret data causes
exceptionally grave damage to the national security, whereas the loss of
Secret data causes only serious damage.  (4)

                            TABLE 3
                  SECURITY RISK INDEX MATRIX

                         Maximum Data Sensitivity

                             U     N     C    S    TS   1C   MC

                      U      0     1     2    3    4    5    6
                      N      0     0     1    2    4    5    6
   Minimum            C      0     0     0    1    3    4    5
   Clearance          S      0     0     0    0    2    3    4
   or
   Authorization    TS(BI)   0     0     0    0    0    2    3
   of
   System Users     TS(SBI)  0     0     0    0    0    1    2
                      1C     0     0     0    0    0    0    1
                      MC     0     0     0    0    0    0    0

U = Uncleared or Unclassified
N = Not Cleared but Authorized Access to Sensitive Unclassified Information or
Not Classified but Sensitive
C = Confidential
S = Secret
TS = Top Secret
TS(BI) = Top Secret (Background Investigation)
TS(SBI) = Top Secret (Special Background Investigation)
1C = One Category
MC = Multiple Categories

In situations where the local environment indicates that additional risk
factors are present, a larger risk index may be warranted.  Table 2 and the
above discussion show how the presence of nonhierarchical sensitivity
categories such as NOFORN (Not Releasable to Foreign Nationals) and PROPIN
(Caution- Proprietary Information Involved) influences the ratings.(14)
Compartmented information is also encompassed by the term sensitivity
categories as is information revealing sensitive intelligence sources and
methods.  A' subcategory (and a subcompartment) is considered to be
independent from the category to which it is subsidiary.

Table 3 presents a matrix summarizing the risk' indices corresponding to the
various clearance/sensitivity pairings. For simplicity no categories are
associated with the maximum data sensitivity levels below Top Secret.

3.0 COMPUTER SECURITY REQUIREMENTS FOR OPEN SECURITY ENVIRONMENTS

This section discusses the application of the Computer Security Requirements
to systems in open security environments. An open security environment is
one in which system applications are not adequately protected against the
insertion of malicious logic.  Appendix C describes malicious logic and the
open security environment in more detail.

3.1 Recommended Classes

Table 4 presents the minimim evaluation class identified in the Computer
Security Requirements for different risk indices in an open security
environment.  Table 5 illustrates the impact of the requirements on individual
minimum clearance/maximum data sensitivity pairings, where no categories are
associated with maximum data sensitivity below Top Secret.  The minimum
evaluation class is determined by finding the matrix entry corresponding to
the minimum clearance or authorization of system users and the maximum
sensitivity of data processed by the system.

     Example: If the minimum clearance of system users is Secret and the
     maximum sensitivity of data processed is Top Secret (with no categories),
     then the risk index is 2 and a class B2 system is required.

The classes identified are minimum values.  Environmental characteristics must
be examined to determine whether a higher class is warranted.  Factors that
might argue for a higher evaluation class include the following:

     a. High volume of information at the maximum data sensitivity.

     b. Large number of users with minimum clearance.

Both of these factors are often present in networks.

The guidance embodied in the Computer Security Requirements is best used
during system requirements definition to determine which class of trusted
system is required given the risk index envisioned for a specific environment.
They are also of use in determining which choices are feasible given either
the maximum sensitivity of data to be processed or minimum user clearance or
authorization requirements. The Computer Security Requirements can also be
used in a security evaluation to determine whether system safeguards are
sufficient.

3.2 Risk index and Operational Modes

Situations with a risk index of zero encompass systems operating in system
high or dedicated mode.  Systems operating in dedicated mode--in which all
users have both the clearance and the need-to-know for all information in the
system--do not need to rely on hardware and software protection measures for
security.(10) Therefore, no minimum level of trust is prescribed.  However,
because of the integrity and denial of service requirements of many systems,
additional protective features may be warranted.

                             TABLE 4

  COMPUTER SECURITY      REQUIREMENTS FOR OPEN SECURITY
                         ENVIRONMENTS

    RISK INDEX         SECURITY OPERATING        MINIMUM CRITERIA
                               MODE                  CLASS1

         0              Dedicated                  No Prescribed
                                                    Minimum2
         0                  System High                C23
         1            Limited Access, Controlled,      B14
                      Compartmented, Multilevel
         2            Limited Access, Controlled,       B2
                      Compartmented, Multilevel
         3               Controlled, Multilevel         B3
         4              Multilevel                      A1
         5              Multilevel                      *
         6              Multilevel                      *
         7              Multilevel                      *

1 The asterisk (*) indicates that computer protection for environments with
that risk index are considered to be beyond the state of current technology.
Such environments must augment technical protection with personnel or
administrative security safeguards.

2 Although there is no prescribed minimum, the integrity and denial of service
requirements of many systems warrant at least class C1 protection.

3 If the system processes sensitive or classified data, at least a class C2
system is required.  If the system does not process sensitive or classified
data, a class C1 system is sufficient.

4 Where a system processes classified or compartmented data and some users do
not have at least a Confidential clearance, or when there are more than two
types of compartmented information being processed, at least a class B2 system
is required.

                            TABLE 5

 SECURITY INDEX MATRIX FOR OPEN SECURITY ENVIRONMENTS1

                Maximum Data Sensitivity

                          U     N     C     S     TS    1C    1M

                    U     C1    B1    B2    B3    *     *     *
     Minimum        N     C1    C2    B2    B2    A1    *     *
     Clearance or   C     C1    C2    C2    B1    B3    A1    *
     Author-
     ization        S     C1    C2    C2    C2    B2    B3    A1
     of System
     Users        TS(BI)  C1    C2    C2    C2    C2    B2    B3

                 TS(SBI)  C1    C2    C2    C2    C2    B1    B2
                   1C     C1    C2    C2    C2    C2    C22   B13
                   MC     C1    C2    C2    C2    C2    C22   C22

1 Environments for which either C1 or C2 is given are for systems that operate
in system high mode.  No minimum level of trust is prescribed for systems that
operate in dedicated mode.  Categories are ignored in the matrix, except for
their inclusion at the TS level.

2 It is assumed that all users are authorized access to all categories present
in the system.  If some users are not authorized for all categories, then a
class B1 system or higher is required.

3 Where there are more than two categories, at least a class B2 system is
required.

U = Uncleared or Unclassified
N = Not Cleared but Authorized Access to Sensitive Unclassified Information or
Not Classified but Sensitive
C = Confidential
S = Secret
TS = Top Secret
TS(BI) = Top Secret (Background Investigation)
TS(SBI) = Top Secret (Special Background Investigation)
1C = One Category
MC = Multiple Category

In system high mode, all users have sufficent security clearances and category
authorizations for all data, but some users do not have a need-to-know for all
information in the system.(10) Systems that operate in system high mode thus
are relied on to protect information from users who do not have the
appropriate need-to-know. Where classified or sensitive unclassified data is
involved, no less than a class C2 system is allowable due to the need for
individual accountability.

In accordance with policy, individual accountability requires that individual
system users be uniquely identified and an automated audit trail kept of their
actions.  Class C2 systems are the lowest in the hierarchy of trusted systems
to provide individual accountability and are therefore required where
sensitive or classified data is involved.  The only case where no sensitive or
classified data is involved is the case in which the maximum sensitivity of
data is unclassified.  In this case, hardware and software controls are
still required to allow users to protect project or private information and to
keep other users from accidentally reading or destroying their data.  However,
since there is no officially sensitive data involved, individual
accountability is not required and a class C1 system suffices.  In system high
mode sensitivity labels are not required for making access control
decisions.  In this mode access is based on the need-to-know, which is based
on permissions (e.g., group A has access to file A), not on sensitivity
labels.  The type of access control used to provide need-to-know protection is
called discretionary access control. It is defined as a means of restricting
access to objects based on the identity of subjects and/or groups to which the
subjects belong.  All systems above Division D provide discretionary access
control mechanisms.  These mechanisms are more finely grained in class C2
systems than in Class C1 systems in that they provide the capability of
including or excluding access to the granularity of a single user.  Division C
systems (C1 and C2) do not possess the capability to provide trusted labels on
output.  Therefore, output from these systems must be labeled at the system
high level and manually reviewed by a responsible individual to determine
the correct sensitivity prior to release beyond the perimeter of the system
high protections of the system.(10)

Environments with a risk index of 1 or higher encompass systems operating in
controlled, compartmented, and multilevel modes.  These environments require
mandatory access control, which is the type of access control used to provide
protection based on sensitivity labels.  It is defined as a means of
restricting access to objects based on the sensitivity (as represented by a
label) of the information contained in the objects and the formal clearance or
authorization of subjects to access information of such sensitivity.  Division
B and A systems provide mandatory access control, and are therefore required
for all environments with risk indices of 1 or greater.

The need for internal labeling has a basis in policy, in that DoD Regulation
5200.1-R requires computer systems that process sensitive or classified data
to provide internal classification markings.(3) Other requirements also exist.

     Example: The DCID entitled "Security Controls on the Dissemination of
     Intelligence Information" requires that security control markings be
     "associated (in full or abbreviated form) with data stored or processed
     in automatic data processing systems."(14)

Sensitivity labeling is also required for sensitive unclassified data.(15,16)

     Example: Data protected by Freedom of Information (FOI) Act exemptions
     must be labeled as being "exempt from mandatory disclosure under the FOI
     Act."(15)

This example illustrates not only the need for labeling but also the fact that
the purpose of FOI Act exemptions is to provide access control protection for
sensitive data.  In summary, it is a required administrative security practice
that classified and unclassified sensitive information be labeled and
controlled based on the labels.  It follows that prudent computer security
practice requires similar labeling and mandatory access control.

The minimum class recommended for environments requiring mandatory access
control is class B1, since class B1 systems are the lowest in the hierarchy of
trusted systems to provide mandatory access control.

     Example:  Where no categories are involved, systems with minimum
     clearance/maximum data sensitivity pairings of U/N and C/S have a risk
     index of 1 and thus require at least a class B1 system.

Some systems that operate in system high mode use mandatory access control for
added protection within the system high environment, even though the controls
are not relied upon to properly label and protect data passing out of the
system high environment.  There has also been a recommendation that mandatory
access controls (i.e., class B1 or higher systems) be used whenever data at
two or more sensitivity levels is being processed, even if everyone is fully
cleared, in order to reduce the likelihood of mixing data from files of higher
sensitivity with data of files of lower sensitivity and releasing the data at
the lower sensitivity.(17) These points reaffirm the fact that the classes
identified in the requirements are minimum values.

This report emphasizes that output from a system operating in system high mode
must be stamped with the sensitivity and category labels of the most sensitive
data in the system until the data is examined by a responsible individual and
its true sensitivity level and category are determined.  If a system can only
be trusted for system high operation, its labels cannot be assumed to
accurately reflect data sensitivity.  The use of division B or A systems does
not necessarily solve this problem.

     Example: Take the case of a system in an open security environment that
     processes data classified up to Secret and supports some users who have
     only Confidential clearances.  According to the requirements, such a
     situation represents a risk index of 1 and thus requires a class B1
     system.  Some of the reports produced by the system might be
     unclassified. Nevertheless, such a report cannot be forwarded to
     uncleared people until the report is examined and its contents determined
     to be unclassified. Without the existence of such a review, the recipient
     becomes an indirect user and the risk index becomes 3. A class B1
     system no longer provides adequate data protection. Therefore, even
     though the system is trusted to properly label and segregate Confidential
     and Secret data, it is not simultaneously trusted to properly label and
     segregate unclassified data.

Systems with a risk index of 2 require more trust than can be placed in a
class B1 system.  Where no categories are involved, class B2 systems are the
minimum required for minimum clearance/maximum data sensitivity pairings
such as U/C, N/S and S/TS, all of which have a risk index of 2.  Class B2
systems have several characteristics that justify this increased trust:

     a.  The Trusted Computing Base (TCB) is carefully structured into
         protection-critical and nonprotection-critical elements.  The TCB

         interface is well defined, and the TCB design and implementation
         enable it to be subjected to more thorough testing and more complete
         review.

     b.  The TCB is based on a clearly defined and documented formal security
         policy model that requires the discretionary and mandatory access
         control enforcement found in class B1 systems to be extended to all
         subjects and objects in the system. That is, security rules are more
         rigorously defined and have a greater influence on system design.

     c.  Authentication mechanisms are strengthened, making it more difficult
         for a malicious user or malicious software to improperly intervene in
         the login process.

     d.  Stringent configuration management controls are imposed for life-
         cycle assurance.

     e.  Covert channels are addressed to defend against their exploitation by
         malicious software.(18) A covert channel is a communication channel
         that violates the system's security policy.

Because of these and other characteristics, class B2 systems are relatively
resistant to penetration.  A risk index of 3, however, requires greater
resistance to penetration.  Class B3 systems are highly resistant to
penetration and are the minimum required for situations with a risk index of 3
such as those with minimum clearance/maximum data sensitivity pairings of U/S,
C/TS, S/TS with one category, and TS(BI)/TS with multiple categories.
Characteristics that distinguish class B3 from class B2 systems include the
following:

     a.  The TCB must satisfy the reference monitor requirements that it
         mediate all accesses of subjects to objects, be tamperproof, and be
         small enough to be subjected to analysis and tests.  Much effort is
         thus spent on minimizing TCB complexity.

     b.  Enhancements are made to system audit mechanisms and system
         recovery procedures.

     c.  Security management functions are performed by a security
         administrator rather than a system administrator.

While several new features have been added to class B3 systems, the major
distinction between class B2 and class B3 systems is the increased trust that
can be placed in the TCB of a class B3 system.  The most trustworthy systems
defined by the Criteria are class Al systems.  Class Al systems can be used
for situations with a risk index of 4, such as the following minimum
clearance/maximum data sensitivity pairings: N/TS, C/TS with one category, and
S/TS with multiple categories.  Class Al systems are functionally equivalent
to those in class B3 in that no additional architectural features or policy
requirements are added.  The distinguishing characteristic of systems in this
class is the analysis derived from formal design specification and
verification techniques and the resulting high degree of assurance that the
TCB is correctly implemented.  In addition, more stringent configuration
management is required and procedures are established for securely
distributing the system to sites.

The capability to support systems in open security environments with a risk
index of 5 or greater is considered to be beyond the state-of-the-art.  For
example, technology today does not provide adequate security protection for an
open environment with uncleared users and Top Secret data.  Such environments
must rely on physical, personnel, or information security solutions or on such
technical approaches as periods processing.

4.0 COMPUTER SECURITY REQUIREMENTS FOR CLOSED
    SECURITY ENVIRONMENTS

This section discusses the application of the Computer Security Requirements
to systems in closed security environments.  A closed security environment
is one in which system applications are adequately protected against the
insertion of malicious logic.  Appendix C describes the closed security
environment in more detail.  The main threat to the TCB from applications in
this environment is not malicious logic, but logic containing unintentional
errors that might be exploited for malicious purposes.  As system quality
reaches class B2, the threat from logic containing unintentional errors is
substantially reduced. This reduction permits the placement of increased trust
in class B2 systems due to (1) the increased attention that B2 systems give to
the interface between the application programs and the operating system, (2)
the formation of a more centralized TCB, and (3) the elimination of
penetration flaws.  Nevertheless, the evaluation class of B1 assigned for open
security environments cannot be reduced to a class C1 or C2 in closed security
environments because of the requirement for mandatory access controls.

Table 6 presents the minimum evaluation class identified in the Computer
Security Requirements for different risk indices in a closed security
environment.  The principal difference between the requirements for the open
and closed environments is that in closed environments class B2 systems are
trusted to provide sufficient protection for a greater risk index.  As a
result, environments are supportable that were not supportable in open
situations (e.g., uncleared user on a system processing Top Secret data).
Table 7 illustrates the requirements' impact on individual minimum
clearance/maximum data sensitivity pairings.

                             TABLE 6

COMPUTER SECURITY      REQUIREMENTS FOR CLOSED SECURITY
                       ENVIRONMENTS

  RISK INDEX         SECURITY OPERATING       MINIMUM CRITERIA
                            MODE                   CLASS1

        0                  Dedicated             No Prescribed
                                                  Minimum 2
        0                 System High                C23
        1        Limited Access, Controlled,         B14
                 Compartmented, Multilevel
        2        Limited Access, Controlled          B2
                 Compartmented, Multilevel
        3              Controlled, Multilevel        B2
        4                  Multilevel                B3
        5                  Multilevel                A1
        6                  Multilevel                *
        7                  Multilevel                *

1 The asterisk (*) indicates that computer protection for environments with
that risk index are considered to be beyond the state of current technology.
Such environments must augment technical protection with physical, personnel,
and/or administrative safeguards.

2 Although there is no prescribed minimum, the integrity and denial of service
requirements of many systems warrant at least class C1 protection.

3 If the system processes sensitive or classified data, at least a class C2
system is required.  If the system does not process sensitive or classified
data, a class C1 system is sufficient.

-Where a system processes classified or compartmented data and some users do
not have at least a Confidential clearance, at least a class B2 system is
required.

                             TABLE 7
      SECURITY INDEX MATRIX FOR CLOSED SECURITY ENVIRONMENTS1

                            Maximum Data Sensitivity

                        U     N     C     S     TS    1C    MC

                  U     C1    B1    B2    B2    A1    *     *
   Minimum        N     C1    C2    B1    B2    B3    A1    *
   Clearance or   C     C1    C2    C2    B1    B2    B3    A1
   Author-        S     C1    C2    C2    C2    B2    B2    B3
   ization      TS(BI)  C1    C2    C2    C2    C2    B2    B2
   of System   TS(SBI)  C1    C2    C2    C2    C2    B1    B2
   Users         1C     C1    C2    C2    C2    C2    C22   B13
                 MC     C1    C2    C2    C2    C2    C22   C22

1 Environments for which either C1 or C2 is given are for systems that operate
in system high mode.  There is no prescribed minimum level of trust for
systems that operate in dedicated mode.  Categories are ignored in the matrix,
except for their inclusion at the TS level.

2 It is assumed that all users are authorized access to all categories on the
system. If some users are not authorized for all categories, then a class B1
system or higher is required.

3 Where there are more than two categories, at least a class B2 system is
required.

U = Uncleared or Unclassified
N = Not Cleared but Authorized Access to Sensitive UnclassiFied Information or
Not Classified but Sensitive
C = Confidential
S = Secret
TS = Top Secret
TS(BI) = Top Secret (Background Investigation)
TS (SBI) = Top Secret (Special Background Investigation)
1C = One Category
MC = Multiple Categories

                            APPENDIX A

          SUMMARY OF CRITERIA The DoD Trusted Computer System Evaluation
Criteria(4) provides a basis for specifying security requirements and a metric
with which to evaluate the degree of trust that can be placed in a computer
system.  These criteria are hierarchically ordered into a series of evaluation
classes where each class embodies an increasing amount of trust.  A summary of
each evaluation class is presented in this appendix.  This summary should not
be used in place of the Criteria.  The evaluation criteria are based on six
fundamental security requirements that deal with controlling access to
information.  These requirements can be summarized as follows:

   a. Security policy--There must be an explicit and well-defined security
      policy enforced by the system.

   b. Marking--Access control labels must be associated with objects.

   c. Identification--Individual subjects must be identified.

   d. Accountability--Audit information must be selectively kept and
      protected so that actions affecting security can be traced to the
      responsible party.

   e. Assurance--The computer system must contain hardware and software
      mechanisms that can be evaluated independently to provide sufficient
      assurance that the system enforces the security policy.

   f. Continuous protection--The trusted mechanisms that enforce the
      security policy must be protected continuously against tampering and
      unauthorized changes.

The evaluation criteria are divided into four divisions--D, C, B, and A;
divisions C, B, and A are further subdivided into classes.  Division D
represents minimal protection, and class A1 is the most trustworthy and
desirable from a computer security point of view.

The following overviews are excerpts from the Criteria:

   Division D: Minimal Protection. This division contains only one class. It
is reserved for those systems that have been evaluated but fail to meet the
requirements for a higher evaluation class.

   Division C: Discretionary Protection. Classes in this division provide for
discretionary (need-to-know) protection and accountability of subjects and the
actions they initiate, through inclusion of audit capabilities.

     Class C1: Discretionary Security Protection.  The TCB of class C1 systems
nominally satisfies the discretionary security requirements by providing
separation of users and data.  It incorporates some form of, credible controls
capable of enforcing access limitations on an individual basis, i.e.,
ostensibly suitable for allowing users to be able to protect project or
private information and to keep other users from accidentally reading or
destroying their data.  The class C I environment is expected to be one of
cooperating users processing data at the same level(s) of sensitivity.

     Class C2: Controlled Access Protection. Systems in this class enforce a
more finely grained discretionary access control than class C1 systems, making
users individually accountable for their actions through logic procedures,
auditing of security-relevant events, and resources encapsulation.

     Division B: Mandatory Protection.  The notion of a TCB that preserves the
integrity of sensitivity labels and uses them to enforce a set of mandatory
access control rules is a major requirement in this division.  Systems in this
division must carry the sensitivity labels with major data structures in the
system.  The system developer also provides the security policy model on which
the TCB is based and furnishes a specification of the TCB.  Evidence must be
provided to demonstrate that the reference monitor concept has been
implemented.

     Class B1: Labeled Security Protection. Class B1 systems require all the
features required for class C2. In addition, an informal statement of the
security policy model, data labeling, and mandatory access control over named
subjects and objects must be present. The capability must exist for accurately
labeling exported information. Any flaws identified by testing must be
removed.

     Class B2: Structured Protection.  In class B2 systems, the TCB is based
on a clearly defined and documented formal security policy model that requires
the discretionary and mandatory access control enforcement found in B1 systems
be extended to all subjects and objects in the system.  In addition, covert
channels are addressed.  The TCB must be carefully structured into
protection-critical and nonprotection-critical elements.  The TCB interface is
well defined and the TCB design and implementation enable it to be subjected
to more thorough testing and more complete review.  Authentication
mechanisms are strengthened, trusted facility management is provided in the
form of support for systems administrator and operator functions, and
stringent configuration management controls are imposed.  The system is
relatively resistant to penetration.

     Class B3: Security Domains. The class B3 TCB must satisfy the reference
monitor requirements that it mediate all accesses of subjects to objects, be
tamperproof, and be small enough to be subjected to analysis and tests. To
this end, the TCB is structured to exclude code not essential to security
policy enforcement, with significant software engineering during TCB design
and implementation directed toward minimizing its complexity.  A security
administrator is supported, audit mechanisms are expanded to signal security-
relevant events, and system recovery procedures are required. The system is
highly resistant to penetration.

     Division A: Verified Protection. This division is characterized by the
use of formal security verification methods to assure that the mandatory and
discretionary security controls employed in the system can effectively protect
the classified and other sensitive information stored or processed by the
system.  Extensive documentation is required to demonstrate that the TCB meets
the security requirements in all aspects of design, development, and
implementation.

   Class A1: Verified Design.  Systems in class A1 are functionally equivalent
to those in class B3 in that no additional architectural features or policy
requirements have been added.  The distinguishing feature of systems in this
class is the analysis derived from formal design specification and
verification techniques and the resulting high degree of assurance that the
TCB is correctly implemented.  This assurance is developmental in nature
starting with a formal model of security policy and a formal top-level
specification (FTLS) of the design.  In keeping with the extensive design
and development analysis of the TCB required of systems in class A1, more
stringent configuration management is required and procedures are
established for securely distributing the system to sites.  A system
security administrator is supported.

                           APPENDIX B

            DETAILED DESCRIPTION OF CLEARANCES AND DATA
                         SENSITIVITIES

This appendix describes in detail the clearances and data sensitivities (e.g.,
classification) introduced in the body of the report.

B.1 Clearances

This section defines increasing levels of clearance or authorization of system
users. System users include not only those users with direct connections to
the system but also those users without direct connections who might receive
output or generate input that is not reliably reviewed for classification by a
responsible individual.

   a. Uncleared (U)--Personnel with no clearance or authorization.
      Permitted access to any information for which there are no specified
      controls, such as openly published information.

   b. Unclassified Information (N)--Personnel who are authorized access to
      sensitive unclassified (e.g., For Official Use Only (FOUO)) information,
      either by an explicit official authorization or by an implicit
      authorization derived from official assignments or responsibilities.(15)

   c. Confidential Clearance (C)--Requires U.S. citizenship and typically
      some limited records checking.(19) In some cases, a National Agency
      Check (NAC) is required (e.g., for U.S. citizens employed by colleges or
      universities).(20)

   d. Secret Clearance (S)--Typically requires a NAC, which consists of
      searching the Federal Bureau of Investigation fingerprint and
      investigative files and the Defense Central Index of Investigations.(19)
      In some cases, further investigation is required.

   e. Top Secret Clearance based on a current Background Investigation
      (TS(BI))--Requires an investigation that consists of a NAC, personal
      contacts, record searches, and written inquiries. A B1 typically
      includes an investigation extending back 5 years, often with a spot
      check investigation extending back 15 years.(19)

   f. Top Secret Clearance based on a current Special Background
      Investigation (TS(SBI))--Requires an investigation that, in addition to
      the investigation for a B1, includes additional checks on the subject's
      immediate family (if foreign born) and spouse and neighborhood
      investigations to verify each of the subject's former residences in the
      United States where he resided six months or more. An SBI typically
      includes an investigation extending back 15 years.(19)

   g. One category (1C)1 - In addition to a TS(SBI) clearance, written
      authorization for access to one category of information is required.
      Authorizations are the access rights granted to a user by a

        responsible individual (e.g., security officer).

    h.  Multiple categories (MC)' - In addition to TS(SBI) clearance, written
        authorization for access to multiple categories of information is
        required.

The extent of investigation required for a particular clearance varies based
both on the background of the individual under investigation and on derogatory
or questionable information disclosed during the investigation.  Identical
clearances are assumed to be equivalent, however, despite differences in the
amount of investigation peformed.

Individuals from non-DoD agencies might be issued DoD clearances if the
clearance obtained in their agency can be equated to a DoD clearance.  For
example, the "Q" and "L" clearances granted by both the Department of Energy
and the Nuclear Regulatory Commission are considered acceptable for issuance
of a DoD industrial personnel security clearance.(20) The "Q" clearance is
considered an authoritative basis for a DoD Top Secret clearance (based on a
B1) and the "L" clearance is considered an authoritative basis for a DoD
Secret clearance.(20)

Foreign individuals might be granted access to classified U.S.  information
although they do not have a U.S. clearance. Access to classified information
by foreign nationals, foreign governments, international organizations, and
immigrant aliens is addressed by National Disclosure Policy, DoD Directive
5230.11, and DoD Regulation 5200.I-R.(3,21,22) The minimum user clearance
rating table applies in such cases if the foreign clearance can be equated to
one of the clearance or authorization levels in the table.

B.2 Data Sensitivities

Increasing levels of data sensitivity are defined as follows:

     a. Unclassified (U)--Data that is not sensitive or classified:  publicly
        releasable information within a computer system. Note that such data
        might still require discretionary access controls to protect it from
        accidental destruction.

     b. Not Classified but Sensitive (N)--Unclassified but sensitive data.
        Much of this is FOUO data, which is that unclassified data that is
        exempt from release under the Freedom of Information Act.(15) This
        includes data such as the following:

        I.  Manuals for DoD investigators or auditors.

     1  These are actually authorizations rather than clearance levels, but
        they are included here to emphasize their importance.

     2. Examination questions and answers used in determination of the
        qualification of candidates for employment or promotion.

     3. Data that a statute specifically exempts from disclosure, such as
        Patent Secrecy data.(23)

     4. Data containing trade secrets or commercial or financial
        information.

     5. Data containing internal advice or recommendations that reflect
        the decision-making process of an agency.(24)

     6. Data in personnel, medical, or other files that, if disclosed, would
        result in an invasion of personal privacy.(25)

     7. Investigative records.

        DoD Directive 5400.7 prohibits any material other than that cited
        in FOI Act exemptions from being considered or marked
        FOUO.(15) One other form of unclassified sensitive data is that
        pertaining to unclassified technology with military application.(16)
        This refers primarily to documents that are controlled under the
        Scientific and Technical Information Program or acquired under
        the Defense Technical Data Management Program.(26,27) In
        addition to specific requirements for protection of particular forms
        of unclassified sensitive data, there are two general mandates. The
        first is Title 18, U.S. Code 1905, which makes it unlawful for any
        office or employee of the U.S. Government to disclose information
        of an official nature except as provided by law, including when such
        information is in the form of data handled by computer
        systems.(28) Official data is data that is owned by, produced by or
        for, or is under the control of the DoD. The second is Office of
        Management and Budget (OMB) Circular A-71, Transmittal
        Memorandum Number I, which establishes requirements for
        Federal agencies to protect sensitive data.(30)

    c.  Confidential (C)--Applied to information, the unauthorized
        disclosure of which reasonably could be expected to cause damage to
        the national security.(3)

     d. Secret (S)--Applied to information, the unauthorized disclosure of
        which reasonably could be expected to cause serious damage to the
        national security.(3)

     e. Top Secret (TS)--Applied to information, the unauthorized disclosure
        of which reasonably could be expected to cause exceptionally grave
        damage to the national security.(3)

     f. One Category (1C)2--Applied to Top Secret Special Intelligence
        information (e.g., Sensitive Compartmented Information (SCI) or
        operational information (e.g., Single Integrated Operational
        Plan/Extremely Sensitive Information (SIOP/ESI)) that requires
        special controls for restrictive handling.(3) Access to such
        information requires authorization by the office responsible for the
        particular compartment.  Compartments also exist at the C and 5 levels
        (see the discussion below).

     g. Multiple Categories (MC)2--Applied to Top Secret Special Intelligence
        or operational information that requires special controls for

        restrictive handling.  This sensitivity level differs from the 1C
        level only in that there are multiple compartments involved.  The
        number can vary from two to many, with corresponding increases in
        the risk involved.

Data sensitivity groupings are not limited to the hierarchical levels
discussed in Section B.2.  Nonhierarchical sensitivity categories such as
NOFORN and PROPIN are also used.(14) Compartmented information is also
included under the term sensitivity categories, as is information revealing
sensitive intelligence sources and methods.  Other sources of sensitivity
categories include (a) the Atomic Energy Act of 1954, (b) procedures based
on International Treaty requirements, and (c) programs for the collection of
foreign intelligence or under the jurisdiction of the National Foreign
Intelligence Advisory Board or the National Communications Security
Subcommittee.(11,32,33,34,35) Such nonhierarchical sensitivity categories
can occur at each hierarchical sensitivity level.

2 These are actually categories rather than classification levels.  They are
included here to emphasize their importance.

                               APPENDIX C

          ENVIRONMENTAL TYPES The amount of computer security required in a
system depends not only on the risk index (Section 2) but also on the nature
of the environment.  The two environmental types of systems defined in this
document are based on whether the applications that are processed by the TCB
are adequately protected against the insertion of malicious logic.  A system
whose applications are not adequately protected is referred to as being in an
open environment.  If the applications are adequately protected, the system is
in a closed environment.  The presumption is that systems in open environments
are more likely to have malicious application than systems in closed
environments.  Most systems are in open environments.

Before defining the two environmental categories in more detail, it is
necessary to define several terms.

   a. Environment. The aggregate of external circumstances, conditions,
      and objects that affect the development, operation, and maintenance of
      a system.

   b. Application. Those portions of a system, including portions of the
      operating system, that are not responsible for enforcing the systems
      security policy.

   c. Malicious Logic. Hardware, software, or firmware that is intentionally
      included for the purpose of causing loss or harm (e.g., Trojan horses).

   d. Configuration Control. Management of changes made to a system's
      hardware, software, firmware, and documentation throughout the
      development and operational life of the system.

C.1 Open Security Environment

Based on these definitions, an open security environment includes those
systems in which either of the following conditions holds true:

   a. Application developers (including maintainers) do not have sufficient
      clearance (or authorization) to provide an acceptable presumption that
      they have not introduced malicious logic. Sufficient clearance is
      defined as follows: where the maximum classification of data to be
      processed is Confidential or below, developers are cleared and
      authorized to the same level as the most sensitive data; where the
      maximum classification of data to be processed is Secret or above,
      developers have at least a Secret clearance.

   b. Configuration control does not provide sufficient assurance that
      applications are protected against the introduction of malicious logic
      prior to or during the operation of system applications.

Configuration control, by the broad definition above, encompasses all factors
associated with the management of changes to a system.  For example, it
includes the factor that the application's user interface might present a
sufficiently extensive set of user capabilities such that the user cannot be
prevented from entering malicious logic through the interface itself.

In an open security environment, the malicious application logic that is
assumed to be present can attack the TCB in two ways.  First, it can attempt
to thwart TCB controls and thereby "penetrate" the system.  Secondly, it can
exploit covert channels that might exist in the TCB.  This distinction is
important in understanding the threat and how it is addressed by the features
and assurances in the Criteria.

C.2 Closed Security Environment

A closed security environment includes those systems in which both of the
following conditions hold true:

     a. Applications developers (including maintainers) have sufficient
        clearances and authorizations to provide an acceptable presumption
        that they have not introduced malicious logic.

     b. Configuration control provides sufficient assurance that applications
        are protected against the introduction of malicious logic prior to and
        during the operation of system applications.

Clearances are required for assurance against malicious applications logic
because there are few other tools for assessing the security-relevant behavior
of application hardware and software.  On the other hand, several assurance
requirements from the Criteria help to provide confidence that the TCB does
not contain malicious logic.  These assurance requirements include extensive
functional testing, penetration testing, and correspondence mapping between a
security model and the design.  Application logic typically does not have such
stringent assurance requirements.  Indeed, typically it is not practical to
build all application software to the same standards of quality required for
security software.

The configuration control condition implicitly includes the requirement that
users be provided a sufficiently limited set of capabilities to pose an
acceptably low risk of entering malicious logic.  Examples of systems with
such restricted interfaces might include those that offer no data sharing
services and permit the user only to execute predefined processes that run
on his behalf, such as message handlers, transaction processors, and security
"filters" or "guards."

                             GLOSSARY

For additional definitions, refer to the Glossary in the DoD Trusted Computer
System Evaluation Criteria.(4)

Application

   Those portions of a system, including portions of the operating system,
   that are not responsible for enforcing the security policy.

Category

   A grouping of classified or unclassified but sensitive information, to
   which an additional restrictive label is applied (e.g., proprietary,
   compartmented information).

Classification

   A determination that information requires, in the interest of national
   security, a specific degree of protection against unauthorized disclosure
   together with a designation signifying that such a determination has been
   made. (Adapted from DoD Regulation 5200.I-R.)(3) Data classification is
   used along with categories in the calculation of risk index.

Closed Security Environment

   An environment that includes those systems in which both of the following
   conditions hold true:

   a. Application developers (including maintainers) have sufficient
      clearances and authorizations to provide an acceptable presumption
      that they have not introduced malicious logic. Sufficient clearance is
      defined as follows: where the maximum classification of data to be
      processed is Confidential or below, developers are cleared and
      authorized to the same level as the most sensitive data; where the
      maximum classification of data to be processed is Secret or above,
      developers have at least a Secret clearance.

   b. Configuration control provides sufficient assurance that applications
      are protected against the introduction of malicious logic prior to and
      during operation of system applications.

Compartmented Information

   Any information for which the responsible Office of Primary Interest (OPI)
   requires an individual needing access to that information to possess a
   special authorization.

Configuration Control

   Management of changes made to a system's hardware, software, firmware,
   and documentation throughout the developmental and operational life of

   the system.

Covert Channel

   A communications channel that allows a process to transfer information in
   a manner that violates the system's security policy.(4)

Discretionary Access Control

   A means of restricting access to objects based on the identity of subjects
   and/or groups to which they belong. The controls are discretionary in the
   sense that a subject with a certain access permission is capable of passing
   that permission (perhaps indirectly) on to any other subject.(4)

Environment

   The aggregate of external circumstances, conditions, and objects that
   affect the development, operation, and maintenance of a system. (See Open
   Security Environment and Closed Security Environment.)

Label

   Apiece of information that represents the security level of an object and
   that describes the sensitivity of the information in the object.

Malicious Logic

   Hardware, software, or firmware that is intentionally included in a system
   for the purpose of causing loss or harm.

Mandatory Access Control

   A means of restricting access to objects based on the sensitivity (as
   represented by a label) of the information contained in the objects and the
   formal authorization (i.e., clearance) of subjects to access information of
   such sensitivity.(4)

Need-To-Know

   A determination made by the processor of sensitive information that a
   prospective recipient, in the interest of national security, has a
   requirement for access to, knowledge of, or possession of the sensitive
   information in order to perform official tasks or services.  (Adapted from
   DoD Regulation 5220.22-R.)(20)

Open Security Environment

   An environment that includes those systems in which one of the following
   conditions holds true:

   a. Application developers (including maintainers) do not have sufficient
      clearance or authorization to provide an acceptable presumption that
      they have not introduced malicious logic. (See the definition of Closed
      Security Environment for an explanation of sufficient clearance.)

   b. Configuration control does not provide sufficient assurance that
      applications are protected against the introduction of malicious logic
      prior to and during the operation of system applications.

Risk Index

   The disparity between the minimum clearance or authorization of system
   users and the maximum classification of data processed by the system.

Sensitive Information

   Information that, as determined by a competent authority, must be
   protected because its unauthorized disclosure, alteration, loss, or
   destruction will at least cause perceivable damage to someone or
   something.(4)

System

     An assembly of computer hardware, software, and firmware configured for
     the purpose of classifying, sorting, calculating, computing, summarizing,
     transmitting and receiving, storing and retrieving data with a minimum of
     human intervention.

System Users

     Users with direct connections to the system and also those individuals
     without direct connections who receive output or generate input that is
     not reliably reviewed for classification by a responsible individual.
     The clearance of system users is used in the calculation of the risk
     index.

                           ACRONYMS

A1       An evaluation class requiring a verified design
ADP      Automated Data Processing
ADPS     Automated Data Processing System
AFSC     Air Force Systems Command

B1       An Evaluation class requiring labeled security protection
B2       An Evaluation class requiring structured protection
B3       An evaluation class requiring security domains
BI       Background Investigation

C        Confidential
C1       An evaluation class requiring discretionary access protection
C2       An evaluation class requiring controlled access protection
CI       Compartmented Information
CSC      Computer Security Center
COMINT   Communications Intelligence

DCI      Director of Central Intelligence
DCID     Director of Central Intelligence Directive
DIAM     Defense Intelligence Agency Manual
DIS      Defense Investigative Service
DoD      Department of Defense
DoDCSC   Department of Defense Computer Security Center

ESD      Electronic Systems Division

FOI      Freedom of Information
FOUO     For Official Use Only
FTLS     Formal Top-Level Specification

IEEE     Institute of Electrical and Electronics Engineers

L        A personnel security clearance granted by the Department of Energy
         and the Nuclear Regulatory Commission

MC       Multiple Compartments

N        Not Cleared but Authorized Access to Sensitive Unclassified
         Information or Not Classified but Sensitive
NAC      National Agency Check
NATO     North Atlantic Treaty Organization
NOFORN   Not Releasable to Foreign Nationals
NSA      National Security Agency
NSA/CSS  National Security Agency/Central Security Service
NTIS     National Technical Information Service

OMB      Office of Management and Budget
OPI      Office of Primary Interest
OPNAV    Office of the Chief of Naval Operations
OSD      Office of the Secretary of Defense

PRO PIN  Caution--Proprietary Information Involved

Q         A personnel security clearance granted by the Department of Energy
                   and the Nuclear Regulatory Commission

S         Secret
SBI       Special Background Investigation
SCI       Sensitive Compartmented Information
SIOP      Single Integrated Operational Plan
SIOP-ESI  Single Integrated Operational Plan--Extremely Sensitive Information
SM        Staff Memorandum
STD       Standard

TCB       Trusted Computing Base
TS        Top Secret

U         Uncleared or Unclassified
U.S.      United States

IC        One Compartment

                               REFERENCES

1. DoD Computer Security Center, Computer Security Requirements --
   Guidance for Applying the Department of Defense Trusted Computer
   System Evaluation Criteria in Specific Environments, CSC-STD-003-85, 25
   June 1985.

2. DoD Directive 5215.1, "Computer Security Evaluation Center," 25 October
   1982.

3. DoD Regulation 5200.1-R, Information Security Program Regulation,
   August 1982.

4. DoD Computer Security Center, DoD Trusted Computer System Evaluation
   Criteria, CSC-STD-001-83, IS August 1983.

5. Army Regulation 380-380, Automated Systems Security, IS June 1979.

6. Office of the Chief of Naval Operations (OPNAV) Instruction 5239. IA
   "Department of the Navy Automatic Data Processing Security Program," 3'
   August 1982.

7. Air Force Regulation 205-16, Automated Data Processing System (ADPS)
   Security Policy, Procedures, and Responsibilities, I August 1984.

8. Marine Corps Order P5510.14, Marine Corps Automatic Data Processing
   (ADP) Security Manual, 4 November 1982.

9. DoD Directive 5220.22, "DoD Industrial Security Program," 8 December
   1980.

10. DoD Directive 5200.28, "Security Requirements for Automatic Data
    Processing Systems," 29 April 1978.

11. DoD Manual 5200.28-M, ADP Security Manual - Techniques and
    Procedures for Implementing, Deactivating, Testing, and Evaluating
    Secure Resource-Sharing ADP Systems, 25 June 1979.

12. Defense Intelligence Agency Manual (DIAM) 50-4, "Security of
    Compartmented Computer Operations (U)," 24 June 1980,
    CONFIDENTIAL.

13. National Security Agency/Central Security Service (NSA/CSS) Directive
    10-27, "Security Requirements for Automatic Data Processing (ADP)
    Systems," 29 March 1984.

14. Director of Central Intelligence Directive (DCID), "Security Controls on
    the Dissemination of Intelligence Information (U)," 7 January 1984,
    CONFIDENTIAL.

15. DoD Directive 5400.7, "DoD Freedom of Information Act Program," 24
    April 1980.

16.  Office of the Secretary of Defense (OSD) Memorandum, "Control of
     Unclassified Technology with Military Application," 18 October 1983.

17.  Anderson, James P., "An Approach to Identification of Minimum TCB
     Requirements for Various Threat/Risk Environments," Proceedings of the
     1983 IEEE Symposium on Security and Privacy, 24-27 April 1983.

18.  Schell, Roger R., "Evaluating Security Properties of Systems,"
     Proceedings of the IEEE Symposium on Security and Privacy, 24-27 April
     1983.

19.  Defense Investigative Service (DIS) Manual 20-1, Manual for Personnel
     Security Investigations, 30 January 1981.

20.  DoD Regulation 5220.22-R, Industrial Security Regulation, January 1983.

21.  National Disclosure Policy - I, 9 September 1981.

22.  DoD Directive 5230.11, "Disclosure of Classified Military Information to
     Foreign Governments and International Organizations," 31 December
     1976.

23.  Title 35, United States Code, Section 181-188, "Patent Secrecy."

24.  Title 5, United States Code, Section 551, "Administrative Procedures
     Act."

25.  DoD Directive 5400.11, "Department of Defense Privacy Program," 9 June
     1982.

26.  DoD Directive 5100.36, "Defense Scientific and Technical Information
     Program," 2 October 1981.

27.  DoD Directive 5010.12, "Management of Technical Data," 5 December
     1968.

28.  Title 18, United States Code, Section 1905, "Disclosure of Confidential
     Information Generally."

29.  DoD Directive 5200.1, "DoD Information Security Program," 7 June 1982.

30.  Office of Management and Budget (OMB) Circular No. A-71, Transmittal
     Memorandum No. I, "Security of Federal Automated Information Systems,
     27 July 1978.

31.  Joint Chiefs of Staff (JCS) Staff Memorandum (SM) 313-83, Safeguarding
     the Single Integrated Operational Plan (SIOP) (U), 10 May 1983, SECRET.

32.  "Security Policy on Intelligence Information in Automated Systems and
     Networks (U)," Promulgated by the DCI, 4 January 1983,  CONFIDENTIAL.

33.  Director of Central Intelligence Computer Security Manual (U), Prepared
     for the DCI by the Security Committee, 4 January 1983, CONFIDENTIAL.

34.  DoD Directive 5210.2, "Access to and Dissemination of Restricted Data,"
     12 January 1978.

35.  DoD Instruction C-5210.21, "Implementation of NATO Security Procedure
     (U)," 17 December 1973, CONFIDENTIAL.